**12:05:07:05.  Truck approach at point of loading.** The truck approach at the point of loading shall be graded and surfaced to prevent the pooling of water and to effectively protect the milk conducting hose from contamination. The area shall be provided with a concrete slab not less than four feet by eight feet centrally located adjacent to and below the port opening. The truck approach may not be located in a yard, walkway, or holding area where cattle can congregate.

 **Source:** SL 1975, ch 16, § 1; 12 SDR 128, 12 SDR 154, effective July 1, 1986; 25 SDR 85, effective December 20, 1998; 28 SDR 177, effective June 27, 2002.

 **General Authority:** SDCL 39-6-9.

 **Law Implemented:** SDCL 39-6-9(9).