**44:02:08:08.  Heating equipment.** Each facility shall have a heating system capable of maintaining a temperature between 65 degrees Fahrenheit and 75 degrees Fahrenheit. Any heating equipment, if fuel-burning, shall be inspected at least once a year by a person in the business of heating system maintenance (which includes hot water heaters, primary heating sources, and secondary heating sources). A written verification of the inspection must be kept on file in the facility with the date of inspection, a written statement by the person making the inspection, and that person's signature.

 **Source:** 34 SDR 321, effective June 30, 2008.

 **General Authority:** SDCL 34-1-17, 34-18-22.

 **Law Implemented:** SDCL 34-18-22, 34-18-24.

 **Cross-Reference:** 2006 International Building Code, ch 12, sec 1204.