**44:02:08:17.  Egress window exception.** For lodging establishments constructed before July 1, 2009, each grade level egress window shall have at least a net clear opening of five square feet and shall be at least 24 inches high and at least 20 inches wide.

**Source:** 36 SDR 96, effective December 8, 2009.

**General Authority:** SDCL 34-1-17, 34-18-22.

**Law Implemented:** SDCL 34-18-22, 34-18-22.1, 34-18-22.2, 34-18-24.