**44:03:01:08.07.  Equipment standards for mobile X ray equipment.** In addition to § 44:03:01:08.02, mobile X ray equipment must have the exposure switch located so the operator can stand at least six feet from the useful beam. If sufficient shielding is provided to protect the operator from stray radiation, in which case the exposure switch may be located closer.

 **Source:** 26 SDR 96, effective January 23, 2000; 50 SDR 41, effective October 11, 2023.

 **General Authority**: SDCL 34-21-4.1, 34-21-15.

 **Law Implemented:** SDCL 34-21-4.1.