**CHAPTER 61:08:09**

**HISTORIC POWER BOILERS**

Section

61:08:09:01 Definitions.

61:08:09:02 Schedule of inspections.

61:08:09:03 Inspection fees.

61:08:09:04 Appeal from decision by inspector.

61:08:09:05 Internal inspection of boilers.

61:08:09:06 Preparation of boiler for internal inspection.

61:08:09:07 Internal inspection -- Openings.

61:08:09:08 Internal inspection -- Evidence of overheating.

61:08:09:09 Internal inspection -- Condition of flues.

61:08:09:10 Internal inspection -- Checking for cracks.

61:08:09:11 Internal inspection -- Extent of corrosion.

61:08:09:12 Internal inspection -- Test of staybolts.

61:08:09:13 Maximum allowable working pressure.

61:08:09:14 Requirements for hydrostatic pretest.

61:08:09:15 Hydrostatic pretest -- Pipe requirements.

61:08:09:16 Hydrostatic pretest -- Steam gauge connections.

61:08:09:17 Hydrostatic pretest -- Steam gauge capacity.

61:08:09:18 Hydrostatic pretest -- Safety valve requirements.

61:08:09:19 Hydrostatic pretest -- Steam outlet requirements.

61:08:09:20 Hydrostatic pretest -- Blowoff valve requirements.

61:08:09:21 Hydrostatic pretest -- Feed water pipe requirements.

61:08:09:22 Hydrostatic pretest -- Feed water supply.

61:08:09:23 Hydrostatic pretest -- Water level indicator.

61:08:09:24 Requirements to perform hydrostatic test.

61:08:09:25 Required hydrostatic test pressure.

61:08:09:26 Hydrostatic test -- Required water temperature.

61:08:09:27 Hydrostatic test -- Safety valve and steam gauge requirements.

61:08:09:28 Duration of hydrostatic test.

61:08:09:29 Ultrasonic examination for thickness determination.

61:08:09:30 Internal inspection report.

61:08:09:31 External inspections and tests.

61:08:09:32 Preparation of boiler for external inspection.

61:08:09:33 External inspection -- Cleanliness and ASME code compliance.

61:08:09:34 External inspection -- Evidence of leakage.

61:08:09:35 External inspection -- Water glass requirements.

61:08:09:36 External inspection -- Safety valve requirements.

61:08:09:37 External inspection -- Blowoff piping requirements.

61:08:09:38 External inspection report.

61:08:09:39 Repairs to historic power boilers.

61:08:09:40 Minor repairs.

61:08:09:41 Major repairs.

61:08:09:42 Tests following major repairs.

61:08:09:43 Repair methods.

61:08:09:44 Repair of defects.

61:08:09:45 Repair of cracks.

61:08:09:46 Repair of minor cracks and imperfections.

61:08:09:47 Repair of cracks radiating from holes.

61:08:09:48 Repair of welded butt joints.

61:08:09:49 Repair of wasted surfaces.

61:08:09:50 Welding on butt straps.

61:08:09:51 Staybolt replacement.

61:08:09:52 Inspection of welds.

61:08:09:53 Approval of major repairs and report.

61:08:09:54 Requirements for construction of new boilers.

61:08:09:55 Qualifications of inspectors.

Appendix A Guide to Riveted Joint Efficiencies.