**70:07:02:08.  Work classification.** Types of work are classified as follows:

(1)  Major grading;

(2)  Minor grading;

(3)  Portland cement concrete paving;

(4)  Portland cement concrete repair, including spall repair, joint repair, and pavement grinding;

(5)  Asphalt concrete paving and microsurfacing;

(6)  Asphalt surface treatment and asphalt crack sealing;

(7)  New bridge construction;

(8)  Bridge rehabilitation, including deck overlays, fatigue retrofit, steel and concrete repair, and rail retrofit;

(9)  Minor structure construction, including cast in place box culverts, pre-cast multi-beam deck bridges, and mechanically stabilized earth large panel retaining walls;

(10)  Lighting and signals;

(11)  Signing, delineation, and pavement marking;

(12)  Underground work and utilities, including storm sewer, sanitary sewer, waterline, drainage pipe, and precast box culvert;

(13)  Incidental construction, including fencing, guardrail, railroad crossings, mechanically stabilized earth modular block retaining walls, gravel surfacing, base course, landscaping, and erosion control;

(14)  Miscellaneous concrete construction, including sidewalk, bike path, multi-use path, and curb and gutter;

(15)  Bridge painting; and

(16)  High friction surface treatment and bridge deck polymer chip seal.

The committee may approve a prospective bidder in one or more types of work.

The committee may prequalify a prospective bidder on a project by project basis for one or more types of work or specialty work not specifically covered by the foregoing classifications.

**Source:** SL 1975, ch 16, § 1; 8 SDR 45, effective October 28, 1981; 13 SDR 129, 13 SDR 134, effective July 1, 1987; transferred from § 70:01:05:06, 19 SDR 154, effective April 11, 1993; 25 SDR 145, effective May 30, 1999; 40 SDR 121, effective January 6, 2014; 47 SDR 38, effective October 6, 2020.

**General Authority:** SDCL 31-5-10.

**Law Implemented:** SDCL 31-5-10.