**CHAPTER 74:12:04**

**OIL PRODUCTION OPERATING PRACTICES**

Section

74:12:04:01 Gas-oil ratio test required on oil wells -- Procedure.

74:12:04:02 Subsurface pressure tests required on oil wells -- Procedure.

74:12:04:03 Commingling of oil from separate pools prohibited underground.

74:12:04:04 Control of multiple completed wells to ensure segregation of sources required.

74:12:04:05 Vented casinghead gas -- Volume to be measured.

74:12:04:06 Use of vacuum prohibited.

74:12:04:07 Oil to be measured before being sent to collection point.

74:12:04:08 Tank battery meters to be checked -- Reports.

74:12:04:09 Oil storage in open receptacles prohibited -- Fire walls required on oil tanks.

74:12:04:10 Immediate notice by telephone, facsimile, or email required of fire, releases, breaks, leaks, or blowouts.

74:12:04:11 Written follow-up report required.

74:12:04:12 Remediation and disposal of soils contaminated by crude oil.

74:12:04:13 Open burning as remediation alternative.

74:12:04:14 Monthly reports of production required.

74:12:04:15 Disposal of produced water.

74:12:04:16 Approval required for construction of produced water handling facilities.

74:12:04:17 Pits to be constructed and operated to protect certain birds and other species.

74:12:04:18 Transfer of ownership of oil and gas operations.