**74:53:01:26.  Requirements for holding tanks.** The requirements for holding tanks are as follows:

(1)  The minimum liquid holding capacity shall be 1,000 gallons or the wastewater flow generated over a period of 7 days, whichever is greater. There shall be no discharge of effluent from the tank;

(2)  The tank shall be equipped with a high-water alarm positioned to allow at least 3 days of storage after the alarm is activated;

(3)  Holding tanks shall conform to the requirements for septic tanks under subdivisions 74:53:01:23(1) to (3), inclusive, with the exception of outlet devices; and

(4)  Holding tanks shall be installed to meet the requirements for septic tanks under § 74:53:01:24.

**Source:** 12 SDR 2, effective July 18, 1985; 13 SDR 129, 13 SDR 141, effective July 1, 1987; transferred from § 74:03:01:63, July 1, 1996.

**General Authority:** SDCL 34A-2-93.

**Law Implemented:** SDCL 34A-2-20.