**74:53:01:33.  Absorption or alternative water-carriage system permitted under certain circumstances.** An absorption system or alternative water-carriage system may be used when the percolation rate as determined by § 74:53:01:31 or 74:53:01:32 is between 5 and 60 minutes per inch if all other requirements for the absorption system or alternative water-carriage system are met. An alternative water-carriage system must be used when the percolation rate of the soil is slower than 60 minutes per inch or faster than 5 minutes per inch. An absorption system may be used where fill material is used to decrease the percolation rate from more than one but less than 5 minutes per inch to more than 5 but less than 60 minutes per inch.

 **Source:** 12 SDR 2, effective July 18, 1985; 13 SDR 129, 13 SDR 141, effective July 1, 1987; transferred from § 74:03:01:70, July 1, 1996.

 **General Authority:** SDCL 34A-2-93.

 **Law Implemented:** SDCL 34A-2-20, 34A-2-21.