**74:53:01:34.  Seepage pits allowable.** A seepage pit is permissible at the end of an absorption system if the bottom of the pit is no more than 4 feet below the ground surface and the requirements of § 74:53:01:15 and either § 74:53:01:31 or 74:53:01:32 are met.

 **Source:** 12 SDR 2, effective July 18, 1985; 13 SDR 129, 13 SDR 141, effective July 1, 1987; transferred from § 74:03:01:71, July 1, 1996.

 **General Authority:** SDCL 34A-2-93.

 **Law Implemented:** SDCL 34A-2-20, 34A-2-21.