**20:10:36:49.  Tier 3 interconnection completion.** The tier 3 application process is complete when:

(1)  All tier 3 screening criteria are satisfied and any minor modifications to the EDS that may have been identified are implemented;

(2)  The small generator facility installation is approved by an electric code inspector with jurisdiction over the interconnection;

(3)  There is a successful completion of the witness test, if required;

(4)  The parties execute a certificate of completion; and

(5)  An interconnection agreement has been executed.

**Source:** 35 SDR 305, effective July 1, 2009.

**General Authority:** SDCL 49-34A-27, 49-34A-93.

**Law Implemented:** SDCL 49-34A-27, 49-34A-93.