**CHAPTER 74:56:05**

**REMEDIATION CRITERIA FOR PETROLEUM-CONTAMINATED SOILS**

Section

74:56:05:01 Definitions.

74:56:05:02 Exposure pathway defined.

74:56:05:03 Corrective action preceding a Tier 1 assessment.

74:56:05:04 Chemicals of concern.

74:56:05:05 Determination of total petroleum hydrocarbon concentration -- Method.

74:56:05:06 Tier 1 assessments.

74:56:05:07 Tier 1 action levels -- Criteria for calculation.

74:56:05:08 Soils exceeding 500 parts per million total petroleum hydrocarbons.

74:56:05:09 Corrective action or Tier 2 assessment required.

74:56:05:10 Tier 2 assessments.

74:56:05:11 Tier 2 action levels -- Criteria.

74:56:05:12 Corrective action or Tier 3 assessment required.

74:56:05:13 Tier 3 assessments.

74:56:05:14 Tier 3 action levels -- Criteria.

74:56:05:15 Monitoring wells may be required.

74:56:05:16 Free phase product removal required.

74:56:05:17 Corrective action required.

74:56:05:18 Soil remediation or removal requirements.

74:56:05:19 Visibly contaminated soil in the excavation area.

74:56:05:20 Unrecoverable petroleum-contaminated soils.

74:56:05:21 On-site storage of contaminated soils.

74:56:05:22 Off-site storage of contaminated soils.

74:56:05:23 Alternative storage of contaminated soils.

74:56:05:24 Closed-site data base.