**74:51:01:41.  Application of chronic/acute criteria.** Acute and chronic criteria established under § 74:51:01:55 and as translated by Appendix B at the end of this chapter shall be applied as follows:

(1)  Compliance with the chronic criteria or criteria continuous concentration (CCC) is based on the results of a 30-day average. Compliance with CCC in a surface water discharge permit may be based on grab or composite samples;

(2)  Compliance with the acute criteria or criteria maximum concentration (CMC) is based on the results of any one grab sample. However, compliance with CMC in a surface water discharge permit may be based on a composite sample.

**Source:** 19 SDR 111, effective January 31, 1993; transferred from § 74:03:02:32.01, July 1, 1996; 24 SDR 10, effective July 20, 1997.

**General Authority:** SDCL 34A-2-11, 34A-2-93.

**Law Implemented:** SDCL 34A-2-7, 34A-2-11, 34A-2-21.

**Cross-References:** Criteria for toxic pollutants, § 74:51:01:55.