**74:53:01:08.  Wastewater to receive primary treatment prior to discharge to absorption system.** Wastewater shall pass through a septic tank, sedimentation tank, or aerobic system prior to discharge to an absorption system.

**Source:** 12 SDR 2, effective July 18, 1985; 13 SDR 129, 13 SDR 141, effective July 1, 1987; transferred from § 74:03:01:45, July 1, 1996.

**General Authority:** SDCL 34A-2-93.

**Law Implemented:** SDCL 34A-2-20, 34A-2-21.